IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "bim.house catalog product — reference values, verify with manufacturer"
File name: "JPMA-STRUCTURAL-PLYWOOD-WALL.ifc"
Time stamp: "2026-01-01T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 — bim.house product catalog"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE catalog export" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE catalog export" version "1.0" identifier "bim.house" | change ADDED | created 1767225600 (2026-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "構造用合板 耐力壁 (壁倍率2.5) (日本合板工業組合連合会)" | long name "BIM.HOUSE" | phase "Catalog product reference model"
  IFCSITE "Catalog Context" | elevation above sea level 0.
    IFCBUILDING "Catalog Building" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "Level" | elevation 0.
        contains 1 element
          1 x IFCWALL | names: "構造用合板 耐力壁 (壁倍率2.5)" | descriptions: "構造用合板 耐力壁 + 製材軸組 + 高性能GW t105充填断熱 / 壁倍率2.5・準耐火。中庭まわり耐力壁" | property sets: Pset_bimhouse_Catalog

Property sets
  Pset_bimhouse_Catalog | properties | on 1 object (1 IFCWALL)
    ListPrice_JPY_excl_tax = 6000 (IFCINTEGER)
    Manufacturer = "日本合板工業組合連合会" (IFCLABEL)
    ManufacturerURL = "https://www.jpma.jp/" (IFCLABEL)
    Reference = "JPMA-STRUCTURAL-PLYWOOD-WALL" (IFCLABEL)