IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "bim.house catalog product — reference values, verify with manufacturer"
File name: "TESHIKAGA-KUNTAN-INS.ifc"
Time stamp: "2026-01-01T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 — bim.house product catalog"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE catalog export" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE catalog export" version "1.0" identifier "bim.house" | change ADDED | created 1767225600 (2026-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "くん炭充填断熱材（調湿・脱臭） ()" | long name "BIM.HOUSE" | phase "Catalog product reference model"
  IFCSITE "Catalog Context" | elevation above sea level 0.
    IFCBUILDING "Catalog Building" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "Level" | elevation 0.
        contains 1 element
          1 x IFCWALL | names: "くん炭充填断熱材（調湿・脱臭）" | descriptions: "籾殻くん炭を壁体内・床下に充填する自然系断熱・調湿材。弟子屈の籾殻由来。SIPsと併用で寒冷地の付加断熱を構成。" | property sets: Pset_bimhouse_Catalog

Property sets
  Pset_bimhouse_Catalog | properties | on 1 object (1 IFCWALL)
    ListPrice_JPY_excl_tax = 3200 (IFCINTEGER)
    Reference = "TESHIKAGA-KUNTAN-INS" (IFCLABEL)
    ThermalTransmittance_U = 0.04 (IFCREAL)